

Extra work request form

To – cscextraworksandquotes@sanctuary.co.uk

| **Contractor name** | BPM Contracting Services Ltd |
| --- | --- |
| **Property Address** | 54 The Hollows, Wilton, Salisbury, SP2 0JE |
| **Works order number** | 4501455864 |
| **Date & Time original job line was completed** | 01/04/2025 |
| **Extra works SOR code** | 201303 201703  201715  201150 201503 303003 303008 603109 231001 231013  custom for scaffolding |
| **Extra works Description** | VARIATION BELOW TO INCLUDE- Full roof replacement (new felt and battens and new tiles)- Full fascia and soffits replacement (existing are rotten and damaged by worms)  Roof Tile:Renew any plain concrete or clay roof tiles (in groups over 10 No.) and remove waste and debris., Quantity: 52.00 SM, SOR: 201303  Ridge:Renew half round or angled ridge tiles edge bedded onto roofing tiles with solid bedding at butt joints in coloured mortar (1:3) and remove waste and debris., Quantity: 5.00 LM, SOR: 201703  Ridge:Remove and refix any loose ridge tiles edge bedded onto roof tiles and with solid bedding at butt joints in coloured mortar (1:3) and mechanically fixed where necessary., Quantity: -5.00 LM, SOR: 201715  Roof Covering:Extra over any renewal or refixing of roof tiles or slates for renew roofing felt and battens., Quantity: 48.00 SM, SOR: 201150  Verge:Renew verge and mineral fibre undercloak to concrete or clay tiles bedded and pointed in coloured mortar (1:3) including all cutting of tiles and refix or renew stainless steel verge clips and remove waste and debris., Quantity: 9.00 LM, SOR: 201503  Fascia/Barge:Renew fascia or barge with WPB external quality plywood, ne 300mm wide fixed to roof timbers, apply preservative to cut ends, including for any shaping to junction with bargeboard remove and refix rainwater goods and any cabling, adjust roof tiles and felt, renewal of any support battens and all mitred joints and decorate to match existing and remove waste and debris., Quantity: 21.00 LM, SOR: 303003  Soffit:Renew soffit board with WPB plywood ne 300mm wide including renew noggins as necessary fixed to roof timbers and refix cables and decorate to match existing and remove waste and debris., Quantity: 21.00 LM, SOR: 303008  Gutter:Take down any PVCu gutter, remove and refix brackets to fascia and refix gutter to brackets to line and level including all angles, outlets and stop ends and remake all joints., Quantity: 12.00 LM, SOR: 603109  Slate:Remove existing lead or proprietary slate to ne 150mm diameter pipe and replace with 500x500mm lead slate with 200mm high collar to ne 150mm diameter pipe including all labours and remove waste and debris., Quantity: 1.00 NO, SOR: 231001  Flashing:Take off lead flashing, set aside, hack out pointing, clean out groove of brickwork, refix flashing and wedge with lead and repoint in mastic., Quantity: 6.00 LM, SOR: 231013  SCAFFOLDINGAlteration to scaffolding to extend to gable end with hop up., Quantity: 1.00 , SOR: |
| **Price (exc VAT)** | £14595.59 |
| **VAT (20%) (if applicable)** | £2919.12 |
| **Price (inc VAT)** | £17514.71 |